IR Hex Codes – 32800, 33900

|  |  |
| --- | --- |
| **Command** | **Code** |
| Extend Lift (UP) | 0x40 |
| Retract Lift (DOWN) | 0xB0 |
| Stop Lift | 0x10 |
| IR Connection Code | 0x40F7 |